**Enable your I2C Communication**

**Make the wiring**   
mpu9250 Raspberry Pi  
SDA -> SDA

SCL-> SCL

VCC-> 3volt

Gnd -> GND

## How to install.

Go to Terminal

Write following commands

Go to the directory

**$ cd mpu9250**

After Reaching in the Directory

Write the commands mention below

**$ sudo pip install FaBo9Axis\_MPU9250**

After the installation of library just run the python script by typing the command

**$ sudo python program.py**

**So it will show the**

9-Axis sensor data on the screen with the speed of 0.1sec